INTERIOR PRE-FLIGHT CHECKLIST

|  |
| --- |
| FLIGHT STATION |
| CONTROL LOCKS.......................................REMOVED AND STOWED |
| CAUTION: CONSIDER WINDS BEFORE REMOVING CONTROL LOCKS |
| WINDSHIELD.........................................................CHECK CONDITION |
| OXYGEN..........CHECK (MIN 1,000/1,500 FOR CCX) CHECK MASKS |
| TRIM.........................................................................CHECK/SET/ZERO |
| FLAPS........................FLAP HANDLE AND POSTION CORRESPOND |
| PARKING BRAKE.......................................................SET/PUMP FIRM |
| EMERGENCY GEAR CONTROLS............................CHECK STOWED |
| START & SUTO IGN SWITCHED....................................................OFF |
| AVIONIC MASTER...........................................................................OFF |
| ENVIROMENTAL CONTROLS........................................................OFF |
| PROP SYNC.....................................................................................OFF |
| TRANSPONDER............................................................................STBY |
| BATTERY...........................................................................................ON |
| VOLTAGE..........................................................................................CHECK |
| FUEL QUANTITY/CURRENT LIMITERS...........................................CHECK |
| GEAR LIGHTS...................................................................................CHECK |
| THREE GREEN........................................................................CHECK |
| GEAR HANDLE..............................................DEPRESS *HD LT TEST* |
| *WHEELS UP* LIGHT.................................................PRESS TO TEST |
| EXTERIOR LIGHTS...............................................CHECK (AS REQ’D) |
| BATTERY.........................................................................................OFF |
| MALFUNCTION SWITCHES............................................................OFF |
| EMERGENCY EQUIPMENT.......................................................CHECK |
| OXYGEN MASKS |
| FIRE EXTINGUISHER UNDER RIGHT SEAT |
| LIFEVEST |
| CHECK RADAR SECURE IN MOUNTING |
| PASSENGER/CARGO COMPARTMENT |
| WINDOWS..................................................................................CHECK |
| EMERGENCY EXIT..........................................LATCHED AND FLUSH |
| EMERGENCY EQUIPMENT................................. CHECK (AS REQ’D) |
| PAX OXYGEN MASKS, LIFEVEST |
| FIRE EXTINGUISHER |
| RAFT |
| FIRST AID KIT |
| AFT COMPARTMENT...............CHECK ALL LOOSE ITEMS STOWED |